(kicad_sch (version 20230121) (generator eeschema)
  (paper "USLetter")
  (title_block
    (title "Chance of Showers")
    (date "2023-11-26")
    (company "Matthew Epland")
  )
  (lib_symbols
    (symbol "Analog_ADC:MCP3008" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -5.08 13.335 0))
      (property "Value" "MCP3008" (at -5.08 11.43 0))
      (property "Footprint" "" (at 2.54 2.54 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21295d.pdf" (at 2.54 2.54 0))
      (property "ki_keywords" "12bit ADC Reference Single Supply SPI 8CH" (at 0 0 0))
      (property "ki_description" "A/D Converter, 10-Bit, 8-Channel, SPI Interface , 2.7V-5.5V" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm*" (at 0 0 0))
      (symbol "MCP3008_0_0"
        (text "ADC" (at -0.635 1.27 0))
        (text "CNTRL" (at 5.969 -2.921 900))
        (text "MUX" (at -6.35 -1.27 900))
      )
      (symbol "MCP3008_0_1"
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -5.08 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 1.27)
            (xy 3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 8.89)
            (xy -7.62 -11.43)
            (xy -5.08 -10.16)
            (xy -5.08 7.62)
            (xy -7.62 8.89)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -3.175)
            (xy -3.81 -3.175)
            (xy -3.81 -11.43)
            (xy -6.35 -11.43)
            (xy -6.35 -10.795)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 3.175)
            (xy 1.905 -0.635)
            (xy -2.54 -0.635)
            (xy -3.81 1.27)
            (xy -2.54 3.175)
            (xy 1.905 3.175)
          )
          (fill (type none))
        )
        (rectangle (start 3.81 -3.81) (end 6.985 3.81)
          (fill (type none))
        )
        (rectangle (start 12.7 -12.7) (end -12.7 10.16)
          (fill (type background))
        )
      )
      (symbol "MCP3008_1_1"
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "CH0")
          (number "1")
        )
        (pin input line (at 15.24 -5.08 180) (length 2.54)
          (name "~{CS}/SHDN")
          (number "10")
        )
        (pin input line (at 15.24 -2.54 180) (length 2.54)
          (name "Din")
          (number "11")
        )
        (pin output line (at 15.24 0 180) (length 2.54)
          (name "Dout")
          (number "12")
        )
        (pin input clock (at 15.24 2.54 180) (length 2.54)
          (name "CLK")
          (number "13")
        )
        (pin power_in line (at -2.54 -15.24 90) (length 2.54)
          (name "AGND")
          (number "14")
        )
        (pin power_in line (at -2.54 12.7 270) (length 2.54)
          (name "Vref")
          (number "15")
        )
        (pin power_in line (at 5.08 12.7 270) (length 2.54)
          (name "Vdd")
          (number "16")
        )
        (pin input line (at -15.24 5.08 0) (length 2.54)
          (name "CH1")
          (number "2")
        )
        (pin input line (at -15.24 2.54 0) (length 2.54)
          (name "CH2")
          (number "3")
        )
        (pin input line (at -15.24 0 0) (length 2.54)
          (name "CH3")
          (number "4")
        )
        (pin input line (at -15.24 -2.54 0) (length 2.54)
          (name "CH4")
          (number "5")
        )
        (pin input line (at -15.24 -5.08 0) (length 2.54)
          (name "CH5")
          (number "6")
        )
        (pin input line (at -15.24 -7.62 0) (length 2.54)
          (name "CH6")
          (number "7")
        )
        (pin input line (at -15.24 -10.16 0) (length 2.54)
          (name "CH7")
          (number "8")
        )
        (pin power_in line (at 5.08 -15.24 90) (length 2.54)
          (name "DGND")
          (number "9")
        )
      )
    )
    (symbol "Connector:Conn_01x04_Pin" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 5.08 0))
      (property "Value" "Conn_01x04_Pin" (at 0 -7.62 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x04, script generated" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x04_Pin_1_1"
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x20_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J1" (at 1.27 28.3402 0))
      (property "Value" "GPIO" (at 1.27 26.035 0))
      (property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (at -123.19 -24.13 0))
      (property "Datasheet" "" (at -123.19 -24.13 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0))
      (symbol "Conn_02x20_Odd_Even_1_1"
        (rectangle (start -1.27 -25.273) (end 0 -25.527)
          (fill (type none))
        )
        (rectangle (start -1.27 -22.733) (end 0 -22.987)
          (fill (type none))
        )
        (rectangle (start -1.27 -20.193) (end 0 -20.447)
          (fill (type none))
        )
        (rectangle (start -1.27 -17.653) (end 0 -17.907)
          (fill (type none))
        )
        (rectangle (start -1.27 -15.113) (end 0 -15.367)
          (fill (type none))
        )
        (rectangle (start -1.27 -12.573) (end 0 -12.827)
          (fill (type none))
        )
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 15.367) (end 0 15.113)
          (fill (type none))
        )
        (rectangle (start -1.27 17.907) (end 0 17.653)
          (fill (type none))
        )
        (rectangle (start -1.27 20.447) (end 0 20.193)
          (fill (type none))
        )
        (rectangle (start -1.27 22.987) (end 0 22.733)
          (fill (type none))
        )
        (rectangle (start -1.27 24.13) (end 3.81 -26.67)
          (fill (type background))
        )
        (rectangle (start 3.81 -25.273) (end 2.54 -25.527)
          (fill (type none))
        )
        (rectangle (start 3.81 -22.733) (end 2.54 -22.987)
          (fill (type none))
        )
        (rectangle (start 3.81 -20.193) (end 2.54 -20.447)
          (fill (type none))
        )
        (rectangle (start 3.81 -17.653) (end 2.54 -17.907)
          (fill (type none))
        )
        (rectangle (start 3.81 -15.113) (end 2.54 -15.367)
          (fill (type none))
        )
        (rectangle (start 3.81 -12.573) (end 2.54 -12.827)
          (fill (type none))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (rectangle (start 3.81 10.287) (end 2.54 10.033)
          (fill (type none))
        )
        (rectangle (start 3.81 12.827) (end 2.54 12.573)
          (fill (type none))
        )
        (rectangle (start 3.81 15.367) (end 2.54 15.113)
          (fill (type none))
        )
        (rectangle (start 3.81 17.907) (end 2.54 17.653)
          (fill (type none))
        )
        (rectangle (start 3.81 20.447) (end 2.54 20.193)
          (fill (type none))
        )
        (rectangle (start 3.81 22.987) (end 2.54 22.733)
          (fill (type none))
        )
        (pin power_out line (at -5.08 22.86 0) (length 3.81)
          (name "+3.3V")
          (number "1")
        )
        (pin passive line (at 7.62 12.7 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 10.16 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_17")
          (number "17")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_18")
          (number "18")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_19")
          (number "19")
        )
        (pin power_out line (at 7.62 22.86 180) (length 3.81)
          (name "+5V")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_20")
          (number "20")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_21")
          (number "21")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_22")
          (number "22")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_23")
          (number "23")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_24")
          (number "24")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_25")
          (number "25")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_26")
          (number "26")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_27")
          (number "27")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_28")
          (number "28")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_29")
          (number "29")
        )
        (pin passive line (at -5.08 20.32 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 -12.7 180) (length 3.81)
          (name "Pin_30")
          (number "30")
        )
        (pin passive line (at -5.08 -15.24 0) (length 3.81)
          (name "Pin_31")
          (number "31")
        )
        (pin passive line (at 7.62 -15.24 180) (length 3.81)
          (name "Pin_32")
          (number "32")
        )
        (pin passive line (at -5.08 -17.78 0) (length 3.81)
          (name "Pin_33")
          (number "33")
        )
        (pin passive line (at 7.62 -17.78 180) (length 3.81)
          (name "Pin_34")
          (number "34")
        )
        (pin passive line (at -5.08 -20.32 0) (length 3.81)
          (name "Pin_35")
          (number "35")
        )
        (pin passive line (at 7.62 -20.32 180) (length 3.81)
          (name "Pin_36")
          (number "36")
        )
        (pin passive line (at -5.08 -22.86 0) (length 3.81)
          (name "Pin_37")
          (number "37")
        )
        (pin passive line (at 7.62 -22.86 180) (length 3.81)
          (name "Pin_38")
          (number "38")
        )
        (pin power_out line (at -5.08 -25.4 0) (length 3.81)
          (name "GND")
          (number "39")
        )
        (pin passive line (at 7.62 20.32 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 7.62 -25.4 180) (length 3.81)
          (name "Pin_40")
          (number "40")
        )
        (pin passive line (at -5.08 17.78 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 17.78 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 15.24 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 15.24 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Motor:Fan_Tacho_PWM" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "M" (at 2.54 5.08 0))
      (property "Value" "Fan_Tacho_PWM" (at 2.54 -2.54 0))
      (property "Footprint" "" (at 0 0.254 0))
      (property "Datasheet" "http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf" (at 0 0.254 0))
      (property "ki_keywords" "Fan Motor tacho PWM" (at 0 0 0))
      (property "ki_description" "Fan, tacho output, PWM input, 4-pin connector" (at 0 0 0))
      (property "ki_fp_filters" "FanPinHeader*P2.54mm*Vertical* PinHeader*P2.54mm*Vertical* TerminalBlock*" (at 0 0 0))
      (symbol "Fan_Tacho_PWM_0_0"
        (arc (start -5.588 1.524) (mid -5.08 1.0182) (end -4.572 1.524)
          (fill (type none))
        )
        (arc (start -5.08 2.032) (mid -5.4392 1.8832) (end -5.588 1.524)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.032)
            (xy -5.334 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.032)
            (xy -5.207 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.064 2.54)
            (xy -4.064 1.016)
            (xy -3.302 1.016)
          )
          (fill (type none))
        )
      )
      (symbol "Fan_Tacho_PWM_0_1"
        (arc (start -2.54 -0.508) (mid 0.0028 0.9121) (end 0 3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.064 2.54)
            (xy -5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0 -4.572)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.2352)
            (xy 0 -2.6416)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 4.2672)
            (xy 0 4.6228)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 4.572)
            (xy 0 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.016)
            (xy -4.064 -1.016)
            (xy -4.064 -2.54)
            (xy -5.08 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.334 -3.302)
            (xy -5.08 -3.302)
            (xy -5.08 -3.048)
            (xy -4.826 -3.048)
            (xy -4.826 -3.302)
            (xy -4.318 -3.302)
            (xy -4.318 -3.048)
            (xy -4.064 -3.048)
            (xy -4.064 -3.302)
            (xy -3.556 -3.302)
          )
          (fill (type none))
        )
        (circle (center 0 1.016) (radius 3.2512)
          (fill (type none))
        )
        (arc (start 0 3.81) (mid 0.053 0.921) (end 2.54 -0.508)
          (fill (type none))
        )
        (arc (start 2.54 -0.508) (mid 0 1.0618) (end -2.54 -0.508)
          (fill (type none))
        )
      )
      (symbol "Fan_Tacho_PWM_1_1"
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "+")
          (number "2")
        )
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "Tacho")
          (number "3")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "PWM")
          (number "4")
        )
      )
    )
    (symbol "Sensor_Pressure:40PC250G" (pin_numbers hide) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -10.16 6.35 0))
      (property "Value" "40PC250G" (at 6.35 6.35 0))
      (property "Footprint" "" (at 2.54 0 0))
      (property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832" (at 2.54 0 0))
      (property "ki_keywords" "gage gauge pressure sensor" (at 0 0 0))
      (property "ki_description" "Gauge pressure sensor, 0 to 250PSI, 5V supply, 0.2% accuracy, integrated signal conditioning, excellent media compatibility" (at 0 0 0))
      (symbol "40PC250G_0_1"
        (circle (center -5.842 1.524) (radius 2.6162)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.112 0.254)
            (xy -4.572 2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.842 -1.27)
            (xy -5.842 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.572 2.794)
            (xy -4.826 1.778)
            (xy -5.588 2.54)
            (xy -4.572 2.794)
          )
          (fill (type outline))
        )
        (rectangle (start 7.62 5.08) (end -10.16 -5.08)
          (fill (type background))
        )
      )
      (symbol "40PC250G_1_1"
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "Vcc")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin output line (at 10.16 0 180) (length 2.54)
          (name "Vout")
          (number "3")
        )
        (pin no_connect line (at -7.62 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "4")
        )
        (pin no_connect line (at -5.08 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "5")
        )
        (pin no_connect line (at -2.54 -5.08 90) (length 2.54) hide
          (name "NC")
          (number "6")
        )
      )
    )
    (symbol "Switch:SW_SPST" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 3.175 0))
      (property "Value" "SW_SPST" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "switch lever" (at 0 0 0))
      (property "ki_description" "Single Pole Single Throw (SPST) switch" (at 0 0 0))
      (symbol "SW_SPST_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.524 1.778)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_SPST_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "power:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+3.3V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3V\"" (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 193.04 81.28) (diameter 1.016) (color 0 0 0 0))
  (junction (at 190.5 96.52) (diameter 1.016) (color 0 0 0 0))
  (junction (at 74.93 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 172.72 129.54) (diameter 1.016) (color 0 0 0 0))
  (junction (at 172.72 111.76) (diameter 1.016) (color 0 0 0 0))
  (junction (at 190.5 121.92) (diameter 1.016) (color 0 0 0 0))
  (junction (at 226.06 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 190.5 116.84) (diameter 1.016) (color 0 0 0 0))
  (junction (at 190.5 104.14) (diameter 1.016) (color 0 0 0 0))
  (junction (at 125.73 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 74.93 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 170.18 81.28) (diameter 1.016) (color 0 0 0 0))
  (no_connect (at 214.63 88.9))
  (no_connect (at 146.05 96.52))
  (no_connect (at 214.63 111.76))
  (no_connect (at 58.42 116.84))
  (no_connect (at 58.42 114.3))
  (no_connect (at 146.05 119.38))
  (no_connect (at 58.42 109.22))
  (no_connect (at 214.63 91.44))
  (no_connect (at 146.05 114.3))
  (no_connect (at 146.05 88.9))
  (no_connect (at 146.05 121.92))
  (no_connect (at 214.63 109.22))
  (no_connect (at 58.42 119.38))
  (no_connect (at 214.63 119.38))
  (no_connect (at 58.42 111.76))
  (no_connect (at 146.05 99.06))
  (no_connect (at 214.63 127))
  (no_connect (at 146.05 93.98))
  (no_connect (at 58.42 121.92))
  (no_connect (at 58.42 106.68))
  (no_connect (at 146.05 127))
  (no_connect (at 214.63 114.3))
  (no_connect (at 214.63 124.46))
  (no_connect (at 214.63 101.6))
  (no_connect (at 214.63 129.54))
  (no_connect (at 214.63 106.68))
  (wire (pts (xy 41.91 93.98) (xy 41.91 96.52)))
  (wire (pts (xy 172.72 111.76) (xy 172.72 129.54)))
  (wire (pts (xy 187.96 111.76) (xy 214.63 111.76)))
  (wire (pts (xy 175.26 93.98) (xy 146.05 93.98)))
  (wire (pts (xy 190.5 86.36) (xy 190.5 96.52)))
  (wire (pts (xy 190.5 104.14) (xy 187.96 104.14)))
  (wire (pts (xy 190.5 116.84) (xy 190.5 121.92)))
  (wire (pts (xy 115.57 140.97) (xy 125.73 140.97)))
  (wire (pts (xy 190.5 104.14) (xy 190.5 116.84)))
  (wire (pts (xy 187.96 88.9) (xy 214.63 88.9)))
  (wire (pts (xy 172.72 91.44) (xy 172.72 111.76)))
  (wire (pts (xy 172.72 91.44) (xy 175.26 91.44)))
  (wire (pts (xy 125.73 140.97) (xy 125.73 124.46)))
  (wire (pts (xy 124.46 106.68) (xy 175.26 106.68)))
  (wire (pts (xy 187.96 109.22) (xy 214.63 109.22)))
  (wire (pts (xy 41.91 111.76) (xy 41.91 114.3)))
  (wire (pts (xy 71.12 132.08) (xy 71.12 127)))
  (wire (pts (xy 172.72 111.76) (xy 175.26 111.76)))
  (wire (pts (xy 240.03 81.28) (xy 240.03 83.82)))
  (wire (pts (xy 78.74 127) (xy 78.74 132.08)))
  (wire (pts (xy 187.96 99.06) (xy 226.06 99.06)))
  (wire (pts (xy 226.06 88.9) (xy 226.06 99.06)))
  (wire (pts (xy 78.74 132.08) (xy 74.93 132.08)))
  (wire (pts (xy 187.96 129.54) (xy 214.63 129.54)))
  (wire (pts (xy 172.72 129.54) (xy 172.72 133.35)))
  (wire (pts (xy 146.05 96.52) (xy 175.26 96.52)))
  (wire (pts (xy 170.18 77.47) (xy 170.18 81.28)))
  (wire (pts (xy 226.06 109.22) (xy 226.06 111.76)))
  (wire (pts (xy 121.92 114.3) (xy 121.92 104.14)))
  (wire (pts (xy 240.03 96.52) (xy 240.03 100.33)))
  (wire (pts (xy 190.5 121.92) (xy 187.96 121.92)))
  (wire (pts (xy 111.76 86.36) (xy 175.26 86.36)))
  (wire (pts (xy 170.18 101.6) (xy 175.26 101.6)))
  (wire (pts (xy 114.3 83.82) (xy 175.26 83.82)))
  (wire (pts (xy 193.04 81.28) (xy 193.04 83.82)))
  (wire (pts (xy 106.68 91.44) (xy 106.68 83.82)))
  (wire (pts (xy 190.5 96.52) (xy 190.5 104.14)))
  (wire (pts (xy 187.96 93.98) (xy 232.41 93.98)))
  (wire (pts (xy 190.5 96.52) (xy 187.96 96.52)))
  (wire (pts (xy 193.04 77.47) (xy 193.04 81.28)))
  (wire (pts (xy 78.74 99.06) (xy 78.74 93.98)))
  (wire (pts (xy 146.05 88.9) (xy 175.26 88.9)))
  (wire (pts (xy 187.96 81.28) (xy 193.04 81.28)))
  (wire (pts (xy 170.18 81.28) (xy 170.18 101.6)))
  (wire (pts (xy 187.96 101.6) (xy 214.63 101.6)))
  (wire (pts (xy 187.96 91.44) (xy 214.63 91.44)))
  (wire (pts (xy 114.3 91.44) (xy 114.3 83.82)))
  (wire (pts (xy 146.05 99.06) (xy 175.26 99.06)))
  (wire (pts (xy 111.76 91.44) (xy 111.76 86.36)))
  (wire (pts (xy 71.12 93.98) (xy 71.12 99.06)))
  (wire (pts (xy 146.05 119.38) (xy 175.26 119.38)))
  (wire (pts (xy 187.96 83.82) (xy 193.04 83.82)))
  (wire (pts (xy 74.93 91.44) (xy 74.93 93.98)))
  (wire (pts (xy 125.73 124.46) (xy 175.26 124.46)))
  (wire (pts (xy 226.06 101.6) (xy 226.06 99.06)))
  (wire (pts (xy 187.96 124.46) (xy 214.63 124.46)))
  (wire (pts (xy 187.96 119.38) (xy 214.63 119.38)))
  (wire (pts (xy 172.72 129.54) (xy 175.26 129.54)))
  (wire (pts (xy 146.05 114.3) (xy 175.26 114.3)))
  (wire (pts (xy 187.96 127) (xy 214.63 127)))
  (wire (pts (xy 88.9 109.22) (xy 175.26 109.22)))
  (wire (pts (xy 190.5 86.36) (xy 187.96 86.36)))
  (wire (pts (xy 146.05 127) (xy 175.26 127)))
  (wire (pts (xy 52.07 104.14) (xy 58.42 104.14)))
  (wire (pts (xy 97.79 140.97) (xy 105.41 140.97)))
  (wire (pts (xy 88.9 116.84) (xy 175.26 116.84)))
  (wire (pts (xy 124.46 111.76) (xy 124.46 106.68)))
  (wire (pts (xy 125.73 140.97) (xy 130.81 140.97)))
  (wire (pts (xy 190.5 121.92) (xy 190.5 133.35)))
  (wire (pts (xy 74.93 93.98) (xy 71.12 93.98)))
  (wire (pts (xy 187.96 106.68) (xy 214.63 106.68)))
  (wire (pts (xy 175.26 121.92) (xy 146.05 121.92)))
  (wire (pts (xy 88.9 111.76) (xy 124.46 111.76)))
  (wire (pts (xy 190.5 116.84) (xy 187.96 116.84)))
  (wire (pts (xy 232.41 88.9) (xy 226.06 88.9)))
  (wire (pts (xy 170.18 81.28) (xy 175.26 81.28)))
  (wire (pts (xy 74.93 132.08) (xy 71.12 132.08)))
  (wire (pts (xy 88.9 114.3) (xy 121.92 114.3)))
  (wire (pts (xy 109.22 91.44) (xy 109.22 83.82)))
  (wire (pts (xy 121.92 104.14) (xy 175.26 104.14)))
  (wire (pts (xy 187.96 114.3) (xy 214.63 114.3)))
  (wire (pts (xy 78.74 93.98) (xy 74.93 93.98)))
  (wire (pts (xy 138.43 140.97) (xy 140.97 140.97)))
  (wire (pts (xy 74.93 132.08) (xy 74.93 133.35)))
  (label " ID_SDA" (at 146.05 114.3 0) (fields_autoplaced))
  (label " GPIO6" (at 146.05 119.38 0) (fields_autoplaced))
  (label "ID_SCL " (at 214.63 114.3 180) (fields_autoplaced))
  (label " GPIO5" (at 146.05 116.84 0) (fields_autoplaced))
  (label "SDA" (at 114.3 91.44 90) (fields_autoplaced))
  (label "GPIO21{slash}PCM.DOUT " (at 214.63 129.54 180) (fields_autoplaced))
  (label " GPIO19{slash}PCM.FS" (at 146.05 124.46 0) (fields_autoplaced))
  (label " GPIO10{slash}SPI0.MOSI" (at 146.05 104.14 0) (fields_autoplaced))
  (label " GPIO9{slash}SPI0.MISO" (at 146.05 106.68 0) (fields_autoplaced))
  (label "GPIO23 " (at 214.63 99.06 180) (fields_autoplaced))
  (label " GPIO4{slash}GPCLK0" (at 146.05 88.9 0) (fields_autoplaced))
  (label " GPIO27" (at 146.05 96.52 0) (fields_autoplaced))
  (label " GPIO26" (at 146.05 127 0) (fields_autoplaced))
  (label "GPIO14{slash}TXD0 " (at 214.63 88.9 180) (fields_autoplaced))
  (label "GPIO8{slash}SPI0.CE0 " (at 214.63 109.22 180) (fields_autoplaced))
  (label "GPIO15{slash}RXD0 " (at 214.63 91.44 180) (fields_autoplaced))
  (label "GPIO16 " (at 214.63 124.46 180) (fields_autoplaced))
  (label "VCC" (at 109.22 91.44 90) (fields_autoplaced))
  (label " GPIO22" (at 146.05 99.06 0) (fields_autoplaced))
  (label " GPIO2{slash}SDA1" (at 146.05 83.82 0) (fields_autoplaced))
  (label " GPIO17" (at 146.05 93.98 0) (fields_autoplaced))
  (label "GPIO25 " (at 214.63 106.68 180) (fields_autoplaced))
  (label " GPIO3{slash}SCL1" (at 146.05 86.36 0) (fields_autoplaced))
  (label "GPIO18{slash}PCM.CLK " (at 214.63 93.98 180) (fields_autoplaced))
  (label "GPIO12{slash}PWM0 " (at 214.63 119.38 180) (fields_autoplaced))
  (label "GND" (at 106.68 91.44 90) (fields_autoplaced))
  (label " GPIO13{slash}PWM1" (at 146.05 121.92 0) (fields_autoplaced))
  (label "GPIO20{slash}PCM.DIN " (at 214.63 127 180) (fields_autoplaced))
  (label "GPIO24 " (at 214.63 101.6 180) (fields_autoplaced))
  (label "GPIO7{slash}SPI0.CE1 " (at 214.63 111.76 180) (fields_autoplaced))
  (label "SCL" (at 111.76 91.44 90) (fields_autoplaced))
  (label " GPIO11{slash}SPI0.SCLK" (at 146.05 109.22 0) (fields_autoplaced))
  (global_label "+3.3V" (shape input) (at 97.79 140.97 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 89.0249 140.97 0))
  )
  (global_label "GND" (shape input) (at 240.03 100.33 270) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 240.03 107.2808 90))
  )
  (global_label "GND" (shape input) (at 106.68 83.82 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 106.68 76.8692 90))
  )
  (global_label "GND" (shape input) (at 140.97 140.97 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 147.9208 140.97 0))
  )
  (global_label "+5V" (shape input) (at 74.93 91.44 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 74.93 84.4892 90))
  )
  (global_label "GND" (shape input) (at 41.91 114.3 270) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 41.91 121.2508 90))
  )
  (global_label "GND" (shape input) (at 74.93 133.35 270) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 74.93 140.3008 90))
  )
  (global_label "+5V" (shape input) (at 240.03 81.28 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 240.03 74.3292 90))
  )
  (global_label "+5V" (shape input) (at 41.91 93.98 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 41.91 87.0292 90))
  )
  (global_label "+3.3V" (shape input) (at 109.22 83.82 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 109.22 75.0549 90))
  )
  (global_label "+3.3V" (shape input) (at 226.06 111.76 270) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 226.06 120.5251 90))
  )
  (symbol (lib_id "power:+5V") (at 193.04 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR01" (at 193.04 81.28 0))
    (property "Value" "+5V" (at 193.4083 73.1456 0))
    (property "Footprint" "" (at 193.04 77.47 0))
    (property "Datasheet" "" (at 193.04 77.47 0))
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3.3V") (at 170.18 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR04" (at 170.18 81.28 0))
    (property "Value" "+3.3V" (at 170.5483 73.1456 0))
    (property "Footprint" "" (at 170.18 77.47 0))
    (property "Datasheet" "" (at 170.18 77.47 0))
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 190.5 133.35 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR02" (at 190.5 139.7 0))
    (property "Value" "GND" (at 190.6143 137.6744 0))
    (property "Footprint" "" (at 190.5 133.35 0))
    (property "Datasheet" "" (at 190.5 133.35 0))
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 172.72 133.35 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR03" (at 172.72 139.7 0))
    (property "Value" "GND" (at 172.8343 137.6744 0))
    (property "Footprint" "" (at 172.72 133.35 0))
    (property "Datasheet" "" (at 172.72 133.35 0))
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_02x20_Odd_Even") (at 180.34 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J1" (at 181.61 75.7998 0))
    (property "Value" "GPIO" (at 181.61 78.105 0))
    (property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (at 57.15 128.27 0))
    (property "Datasheet" "" (at 57.15 128.27 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "circuit_diagram"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_SPST") (at 110.49 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "SW1" (at 110.49 134.62 0))
    (property "Value" "Hall_Effect_Flow_Switch" (at 110.49 137.16 0))
    (property "Footprint" "" (at 110.49 140.97 0))
    (property "Datasheet" "~" (at 110.49 140.97 0))
    (pin "2")
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "SW1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Sensor_Pressure:40PC250G") (at 41.91 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 30.48 102.87 0))
    (property "Value" "Pressure_Sensor" (at 30.48 105.41 0))
    (property "Footprint" "" (at 44.45 104.14 0))
    (property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832" (at 44.45 104.14 0))
    (pin "6")
    (pin "5")
    (pin "1")
    (pin "2")
    (pin "4")
    (pin "3")
    (instances
      (project "circuit_diagram"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 226.06 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 228.6 104.14 0))
    (property "Value" "1 kΩ" (at 228.6 106.68 0))
    (property "Footprint" "" (at 224.282 105.41 90))
    (property "Datasheet" "~" (at 226.06 105.41 0))
    (pin "2")
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_01x04_Pin") (at 109.22 96.52 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J2" (at 110.49 101.6 90))
    (property "Value" "OLED_I2C_Display" (at 110.49 99.06 90))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (at 109.22 96.52 0))
    (property "Datasheet" "~" (at 109.22 96.52 0))
    (pin "1")
    (pin "4")
    (pin "3")
    (pin "2")
    (instances
      (project "circuit_diagram"
        (path
          (reference "J2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Motor:Fan_Tacho_PWM") (at 240.03 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "F1" (at 245.11 90.17 0))
    (property "Value" "Fan_Tacho_PWM" (at 245.11 92.71 0))
    (property "Footprint" "Connector:FanPinHeader_1x04_P2.54mm_Vertical" (at 240.03 91.186 0))
    (property "Datasheet" "http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf" (at 240.03 91.186 0))
    (pin "2")
    (pin "1")
    (pin "4")
    (pin "3")
    (instances
      (project "circuit_diagram"
        (path
          (reference "F1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Analog_ADC:MCP3008") (at 73.66 111.76 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 80.9341 96.52 0))
    (property "Value" "MCP3008" (at 80.9341 99.06 0))
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (at 76.2 109.22 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21295d.pdf" (at 76.2 109.22 0))
    (pin "8")
    (pin "5")
    (pin "7")
    (pin "16")
    (pin "10")
    (pin "1")
    (pin "6")
    (pin "2")
    (pin "4")
    (pin "9")
    (pin "3")
    (pin "13")
    (pin "11")
    (pin "14")
    (pin "15")
    (pin "12")
    (instances
      (project "circuit_diagram"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 134.62 140.97 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 134.62 134.62 90))
    (property "Value" "10 kΩ" (at 134.62 137.16 90))
    (property "Footprint" "" (at 134.62 142.748 90))
    (property "Datasheet" "~" (at 134.62 140.97 0))
    (pin "2")
    (pin "1")
    (instances
      (project "circuit_diagram"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
